Marlin Heritage 23

STANDARD EQUIPMENT

August 2014

Length Over All 23’ 0”

Length Water Line 16’ 11”

Beam 7’ 7”

Draft 3’ 8 1/4”

Displacement w/inboard 3,845lbs

Ballast 1,400lbs

Sail Area 270sf

Hull:

 \*Solid Hand Laid Fiberglass Hull

 \*Premium White Armorflex Gel Coat Hull Color

 \*Molded Gelcoat Bootstripe

 \*Interlux Fiberglass Bottomkote NT Ablative Bottom Paint – *Owner’s Choice of Colors*

\*Custom One Piece Stainless Steel Rubrail

Deck:

\*Solid Hand Laid Fiberglass Deck

 \*Closed Cell Deck Hardware Reinforcements

 \*Premium White Armorflex Gel Coat Deck Color with Molded Non-Skid

 \*Stunning High Gloss Mahogany Toerails, Coamings, Taffrail & Accents

Keel:

 \*Solid Lead Keel - 1,400lbs

 \*Stainless Steel Keelbolts & Fastening Hardware

 \*Bonded Using Premium Undewater Body Fillers

 \*Seams Filled, Faired & Painted w/ Top Of The Line Interlux Products

Cockpit:

 \*8 Foot Cockpit Seats w/ Lockable Port & Starboard Sail Lockers

 \*Stunning High Gloss Mahogany Coamings

 \*Removable Companionway Doors w/ Smoked Glass & Original Herreshoff Fish Class Hinges

 \*Keyless Engine Panel & Centrally Located Transmission Controls

 \*Dual Purpose Dinette Table w/ Convenient Sail Locker Storage

 \*Cockpit Led Controls for Ease of Sail Handling & Single Handed Sailing

Interior:

 \*Molded Fiberglass Interior Liner w/ Teak Trim Throughout

\*Custom Molded Headliner w/ Attractively Subtle Texture Detail

\*Teak & Holly Floorboards

\*36 Quart Cooler Doubles as Companionway Step

\*2.6 Gallon Porta Potti Located Forward of the Mast on Centerline for Maximum Comfort & Ease of Use

\*7 Foot Long Port & Starboard Settees w/ Plush Low Maintenance Cushions & Storage Below

\*Dual Purpose Dinette Table for Use Below or in the Cockpit w/ Convenient Sail Locker Storage

\*Sound Deadening Insulated Engine Compartment

Cape Cod Shipbuilding Co. \* 7 Narrows Road \* Wareham, MA 02571 \* Phone: (508) 295-3550

Website: www.capecodshipbuilding.com \* Email: info@capecodshipbuilding.com

Deck Hardware:

\*Self -Tacking Jib Traveler System & Roller Furling Hardware by Harken

 \*Carbo Air Blocks and Deck Hardware Throughout by Harken

 \*Herreshoff Manufacturing Company Castings - Cast & Chrome Plated by Edson International

 \*Custom Castings - Cast & Chrome Plated by Edson International

 \*Rope Clutches by Spinlock

 \*Self-Tailing Winches and Winch Handles by Lewmar

 \*Large Flush Mount Deck Hatch w/ Smoke Finish by Lewmar

 \*Custom Hardware by Zephyr Spars

Spars & Rigging: Produced By America’s Longest Running Aluminum Spar Company – Zephyr Spars

 \*Mast :

\*Clear Annodized 6061 T6 Aluminum

\*Modern Rig Design Featuring Aft Swept Spreaders

\*Stainless Steel Standing Rigging Featuring C. Sherman Johnson Turnbuckles & Fittings

\*Premium Double Braid Running Rigging by New England Ropes

\*Cockpit Adjustable Halyard Controls

\*Harken ESP Roller Furler & Complimentary Hardware

\*Harken Carbo Air Blocks & Controls

 \*Boom :

\*Clear Annodized 6061 T6 Aluminum

\*Premium Double Braid Running Rigging by New England Ropes

\*Cockpit Adjustable Single Line Reefing System & Outhaul

\*Harken Carbo Air Blocks & Controls



Steering:

 \*Solid Fiberglass Rudder w/ 1-1/8” Stainless Steel Rudder Shaft

 \*Custom Cast Bronze Rudder Heel Casting & Chrome Plated Rudder Head

 \*Solid, High Luster Varnished Ash Tiller

Electrical:

 \*Recessed Electrical Panel w/ Master On/Off Switch & Spare Room for Additional Circuits

 \*Independent Electric Bilge Pump w/ Automatic Water Level Monitoring

 \*U.S. Coast Guard Approved Navigation Lights

 \*One 12V Marine Grade Battery gell cell

Engine & Propulsion:

\*Yanmar 2YM15 Diesel Inboard Engine w/ Keyless Cockpit Panel

 \* 2 Blade Feathering Propeller

 \*Custom Fuel Tank

Sails & Canvas:

 \*Constructed to Balance Both Performance & Durability by Quantum Sail Group Member – Thurston Sails

 \*Mainsail :

 \*5.93oz High Molecular Weight Woven Polyester

 \*Two Full Length Top Battens

 \*Slug Fed Luff w/ Loose Foot & Reinforced Clew

 \*Includes Tell Tales, Sail Ties & Sail Bag

 \*Self-Tacking Roller Furling Jib

 \*5.93oz High Molecular Weight Woven Polyester w/ UV Protection

\*Includes Tell Tales, Sail Ties & Sail Bag

 \*Sunbrella Mainsail Cover –  *Choice of Colors*

*Proudly Built in Wareham, Massachusetts Since 1899*